Web | This Site

Shared Tutorials New
Website Development
2D & 3D Graphics
Audio & Video Editing
Databases
Desktop Programming
Operating Systems
Business Applications
Miscellaneous
Selected Reading
© 2011 TutorialsPoint.COM

| Top Tutorials |  | New Tutorials |  | Submit |  | Login |  | Register |  | Forums

# Shared Tutorials Directory

Tutorials Shared by the Community

- ### Fixing Avid Xpress underrun adm errors

  In Avid Xpress, an indicator of mismatched sample rates are grey waveforms (sample plots).
  http://www.geniusdv.com/weblog/archives/audio_video_underuns_in_avid_x...

## Tutorial Statistics

- Total Hits: 1438

- Average Rating :

- Total Votes: 0 votes

- Category: Avid XPress Pro/Avid XPress Pro Misc

- Submitted on: 2008-04-16 01:13:51

- Submitted By: Shekhar

- Set as Favorite

## Tutorial Detail ( View Tutorial )

If you are receiving any of the following error messages it is probably because you are using mismatched sample rates within you Avid Xpress project.
AdmAdm Overrun error
AMDConsumer error
Audio Underrun
Video Underrun
Audio files directly from a CD have a sample rate of 44.1. The most common sample rate used for DV media is 48k, or 32k. To keep things simple I suggest always setting your camera to record audio at the 32k sample rate. In your camera, it may give choices for 12 bit audio or 16 bit audio. More detail...
Previous Page

Advertisement

Online Image Processing

Indian Baby Names