Web | This Site

Unix for Beginners
Unix Shell Programming
Advanced Unix
Unix Useful References
Unix Useful Resources
Selected Reading
© 2011 TutorialsPoint.COM

| Home |  | References |  | Discussion Forums |  | About TP

# snmpd - Unix, Linux Command

# NAME

snmpd - daemon to respond to SNMP request packets.

# SYNOPSIS

snmpd [OPTIONS] [LISTENING ADDRESSES]

# DESCRIPTION

snmpd is an SNMP agent which binds to a port and awaits requests from SNMP management software. Upon receiving a request, it processes the request(s), collects the requested information and/or performs the requested operation(s) and returns the information to the sender.

# OPTIONS

Tag | Description
--- | ---
-a | Log the source addresses of incoming requests.
-A | Append to the log file rather than truncating it.
-c FILE | Read FILE as a configuration file (or a comma-separated list of configuration files). Note that the loaded file will only understand snmpd.conf tokens, unless the configuration type is specified in the file as described in the snmp_config man page under SWITCHING CONFIGURATION TYPES IN MID-FILE.
-C | Do not read any configuration files except the ones optionally specified by the -c option. Note that this behaviour also covers the persistent configuration files. This may result in dynamically-assigned values being reset following an agent restart, unless the relevant persistent config files are explicitly loaded using the -c option.
-d | Dump (in hexadecimal) the sent and received SNMP packets.
-D[TOKEN[,...]]
| Turn on debugging output for the given TOKEN(s). Without any tokens specified, it defaults to printing all the tokens (which is equivalent to the keyword "ALL"). You might want to try ALL for extremely verbose output. Note: You can not put a space between the -D flag and the listed TOKENs.
-f | Do not fork() from the calling shell.
-g GID | Change to the numerical group ID GID after opening listening sockets.
-h, --help
| Display a brief usage message and then exit.
-H | Display a list of configuration file directives understood by the agent and then exit.
-I [-]INITLIST
| Specifies which modules should (or should not) be initialized when the agent starts up. If the comma-separated INITLIST is preceded with a ’-’, it is the list of modules that should not be started. Otherwise this is the list of the only modules that should be started.

To get a list of compiled modules, run the agent with the arguments -Dmib_init -H (assuming debugging support has been compiled in).

-L[efos] | Specify where logging output should be directed (standard error or output, to a file or via syslog). See LOGGING OPTIONS in snmpcmd(5) for details.
-m MIBLIST
| Specifies a colon separated list of MIB modules to load for this application. This overrides the environment variable MIBS. See snmpcmd(1) for details.
-M DIRLIST
| Specifies a colon separated list of directories to search for MIBs. This overrides the environment variable MIBDIRS. See snmpcmd(1) for details.
-n NAME | Set an alternative application name (which will affect the configuration files loaded). By default this will be snmpd, regardless of the name of the actual binary.
-p FILE | Save the process ID of the daemon in FILE.
-q | Print simpler output for easier automated parsing.
-r | Do not require root access to run the daemon. Specifically, do not exit if files only accessible to root (such as /dev/kmem etc.) cannot be opened.
-u UID | Change to the user ID UID (which can be given in numerical or textual form) after opening listening sockets.
-U | Instructs the agent to not remove its pid file (see the -p option) on shutdown. Overrides the leave_pidfile token in the snmpd.conf file, see snmpd.conf(5).
-v, --version
| Print version information for the agent and then exit.
-V | Symbolically dump SNMP transactions.
-x ADDRESS
| Listens for AgentX connections on the specified address rather than the default ’/var/agentx/master’. The address can either be a Unix domain socket path, or the address of a network interface. The format is the same as the format of listening addresses described below.
-X | Run as an AgentX subagent rather than as an SNMP master agent.
--name=value
| Allows to specify any token ("name") supported in the snmpd.conf file and sets its value to "value". Overrides the corresponding token in the snmpd.conf file. See snmpd.conf(5) for the full list of tokens.

# LISTENING ADDRESSES

By default, snmpd listens for incoming SNMP requests on UDP port 161 on all IPv4 interfaces. However, it is possible to modify this behaviour by specifying one or more listening addresses as arguments to snmpd. A listening address takes the form:

Tag | Description
--- | ---
| [<transport-specifier>:]<transport-address>

At its simplest, a listening address may consist only of a port number, in which case snmpd listens on that UDP port on all IPv4 interfaces. Otherwise, the <transport-address> part of the specification is parsed according to the following table:

Tag | Description
--- | ---
<transport-specifier> | <transport-address> format
udp (default) | hostname[:port] or IPv4-address[:port]
tcp | hostname[:port] or IPv4-address[:port]
unix | pathname
ipx | [network]:node[/port]
aal5pvc or pvc | [interface.][VPI.]VCI
udp6 or udpv6 or udpipv6
| hostname[:port] or IPv6-address[:port]
tcp6 or tcpv6 or tcpipv6
| hostname[:port] or IPv6-address[:port]

Note that <transport-specifier> strings are case-insensitive so that, for example, "tcp" and "TCP" are equivalent. Here are some examples, along with their interpretation:

Tag | Description
--- | ---
127.0.0.1:161 | listen on UDP port 161, but only on the loopback interface. This prevents snmpd being queried remotely. The port specification ":161" is not strictly necessary since that is the default SNMP port.
TCP:1161 | listen on TCP port 1161 on all IPv4 interfaces.
ipx:/40000 | listen on IPX port 40000 on all IPX interfaces.
unix:/tmp/local-agent | listen on the Unix domain socket /tmp/local-agent.
/tmp/local-agent | is identical to the previous specification, since the Unix domain is assumed if the first character of the <transport-address> is ’/’.
PVC:161 | listen on the AAL5 permanent virtual circuit with VPI=0 and VCI=161 (decimal) on the first ATM adapter in the machine.
udp6:10161 | listen on port 10161 on all IPv6 interfaces.

Note that not all the transport domains listed above will always be available; for instance, hosts with no IPv6 support will not be able to use udp6 transport addresses, and attempts to do so will result in the error "Error opening specified endpoint". Likewise, since AAL5 PVC support is only currently available on Linux, it will fail with the same error on other platforms.

# CONFIGURATION FILES

snmpd checks for the existence of and parses the following files:

Tag | Description
--- | ---
/etc/snmp/snmp.conf
| Common configuration for the agent and applications. See snmp.conf(5) for details.
/etc/snmp/snmpd.conf /etc/snmp/snmpd.local.conf
| Agent-specific configuration. See snmpd.conf(5) for details. These files are optional and may be used to configure access control, trap generation, subagent protocols and much else besides.
| In addition to these two configuration files in /etc/snmp, the agent will read any files with the names snmpd.conf and snmpd.local.conf in a colon separated path specified in the SNMPCONFPATH environment variable.
/usr/share/snmp/mibs/
| The agent will also load all files in this directory as MIBs. It will not, however, load any file that begins with a ’.’ or descend into subdirectories.

# SEE ALSO

snmp_config(5), snmp.conf(5), snmpd.conf(5)

Advertisement

Online Image Processing

Indian Baby Names