Web | This Site

Unix for Beginners
Unix Shell Programming
Advanced Unix
Unix Useful References
Unix Useful Resources
Selected Reading
© 2011 TutorialsPoint.COM

| Home |  | References |  | Discussion Forums |  | About TP

# icclink - Unix, Linux Command

# NAME

icclink - little cms device link generator.

# SYNOPSIS

icclink [options] <profiles>

# DESCRIPTION

lcms is a standalone CMM engine, which deals with the color management. It implements a fast transformation between ICC profiles. icclink is little cms device link generator.

Links two or more profiles into a single devicelink profile. Colorspaces must be paired except Lab/XYZ, that can be interchanged.

# OPTIONS

Tag | Description
--- | ---
-8 | Creates 8-bit devicelink.
-b | Black point compensation.
-c <0,1,2,3>
| Precission (0=LowRes, 1=Normal, 2=Hi-res). [defaults to 1]
-d description
| Description text (quotes can be used).
-h <0,1,2,3>
| Show summary of options and examples.
-i profile
| Input profile (defaults to sRGB).
-k <0..400>
| Ink-limiting in % (CMYK only)
-o profile
| Output devicelink profile. [defaults to ’devicelink.icm’]
-t <0,1,2,3>
| Intent (0=Perceptual, 1=Colorimetric, 2=Saturation, 3=Absolute).
-x | Creatively, guess deviceclass of resulting profile.

| Built-in profiles: *Lab -- D50-based CIEL*a*b (PCS) *XYZ -- CIE XYZ (PCS) *sRGB -- sRGB color space *Gray22- Monochrome of Gamma 2.2 *Lin2222- CMYK linearization of gamma 2.2 on each channel

# EXAMPLES

    To create ’devicelink.icm’ from a.icc to b.icc:
            icclink a.icc b.icc

    To create ’out.icc’ from sRGB to cmyk.icc:
            icclink -o out.icc *sRGB cmyk.icc

    To create a sRGB input profile working in Lab:
            icclink -x -o sRGBLab.icc *sRGB *Lab

    To create a XYZ -> sRGB output profile:
            icclink -x -o sRGBLab.icc *XYZ *sRGB

    To create a abstract profile doing softproof for cmyk.icc:
            icclink -t1 -x -o softproof.icc *Lab cmyk.icc cmyk.icc *Lab

    To create a ’grayer’ sRGB input profile:
            icclink -x -o grayer.icc *sRGB gray.icc gray.icc *Lab

    To embed ink limiting into a cmyk output profile:
            icclink -x -o cmyklimited.icc -k 250 cmyk.icc *Lab

# NOTES

For suggestions, comments, bug reports etc. send mail to info@littlecms.com.

# SEE ALSO

- jpegicc (1)

- tifficc (1)

- icc2ps (1)

- icctrans (1)

- wtpt (1)

This manual page was written by Shiju p. Nair <shiju.p@gmail.com>, for the Debian project.

Advertisement

Online Image Processing

Indian Baby Names