Web | This Site

Unix for Beginners
Unix Shell Programming
Advanced Unix
Unix Useful References
Unix Useful Resources
Selected Reading
© 2011 TutorialsPoint.COM

| Home |  | References |  | Discussion Forums |  | About TP

# showkey - Unix, Linux Command

# NAME

showkey - examine the codes sent by the keyboard

# SYNOPSIS

showkey [-h|--help] [-a|--ascii] [-s|--scancodes] [-k|--keycodes]

# DESCRIPTION

showkey prints to standard output either the scan codes or the keycode or the ‘ascii’ code of each key pressed. In the first two modes the program runs until 10 seconds have elapsed since the last key press or release event, or until it receives a suitable signal, like SIGTERM, from another process. In ‘ascii’ mode the program terminates when the user types ^D.

When in scancode dump mode, showkey prints in hexadecimal format each byte received from the keyboard to the standard output. A new line is printed when an interval of about 0.1 seconds occurs between the bytes received, or when the internal receive buffer fills up. This can be used to determine roughly, what byte sequences the keyboard sends at once on a given key press. The scan code dumping mode is primarily intended for debugging the keyboard driver or other low level interfaces. As such it shouldn’t be of much interest to the regular end-user. However, some modern keyboards have keys or buttons that produce scancodes to which the kernel does not associate a keycode, and, after finding out what these are, the user can assign keycodes with setkeycodes(8).

When in the default keycode dump mode, showkey prints to the standard output the keycode number or each key pressed or released. The kind of the event, press or release, is also reported. Keycodes are numbers assigned by the kernel to each individual physical key. Every key has always only one associated keycode number, whether the keyboard sends single or multiple scan codes when pressing it. Using showkey in this mode, you can find out what numbers to use in your personalized keymap files.

When in ‘ascii’ dump mode, showkey prints to the standard output the decimal, octal, and hexadecimal value(s) of the key pressed, according to he present keymap.

# OPTIONS

Tag | Description
--- | ---
-h --help | showkey prints to the standard error output its version number, a compile option and a short usage message, then exits.
-s --scancodes
| Starts showkey in scan code dump mode.
-k --keycodes
| Starts showkey in keycode dump mode. This is the default, when no command line options are present.
-a --ascii
| Starts showkey in ‘ascii’ dump mode.

# SEE ALSO

- loadkeys (1)

- dumpkeys (1)

- setkeycodes (8)

Advertisement

Online Image Processing

Indian Baby Names